Signal Hound VSG25 App for 64-bit Linux systems

-- Description --
The VSG25 software is used to control the Signal Hound VSG25A vector signal generator.

-- Installation --
To install the software, you can either run the setup script or enter the commands from the script manually.

Superuser privileges are required to run the script/commands, specifically to change the permissions for Signal Hound devices by adding the sh.rules file to /etc/udev/rules.d/.

Run the setup script with:

    chmod 755 setup.sh
    ./setup.sh

-- Usage --
After installation the VSG25 software can be run from the application launcher.

Alternatively, it can be run from a terminal in the application directory with

    ./VSG25

The file 'VSG25' can also be double-clicked in Files, provided that Files is configured to
run executable text files. This setting can be changed as follows:

    Files > Preferences > Behavior > Executable Text Files > Run Them

-- Compilation Notes --
The software was compiled on Ubuntu 18.04 using QtCreator 4.5.2 with Qt 5.9.5 libraries and GCC 7.4.0.

-- Support --
For support contact support@signalhound.com.
